,Voltage##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,Type Comments##OTHER##,Track_Length##LENGTH##MILLIMETERS,Model##OTHER##,Manufacturer##OTHER##,Keynote##OTHER##,FLOS_Main_Finish##OTHER##,Right_Endcap_Visibility##OTHER##,Left_Endcap_Visibility##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES
1000 mm,48.000000000000,http://architectural.flos.com/professional/es/productos/sistemas_generales/the_fast_track,End Caps 08.9070.14 not included. To be ordered separately.,1000.000000000000,06.1850.14,FLOS,26 51 13,FLOS Black Metal Matte,1,1,"Electro-mechanical profile for recessed installations in plasterboard ceilings, with 1m to 3m lengths.",0.000000000000,0.000000000000
2000 mm,48.000000000000,http://architectural.flos.com/professional/es/productos/sistemas_generales/the_fast_track,End Caps 08.9070.14 not included. To be ordered separately.,2000.000000000000,06.1852.14,FLOS,26 51 13,FLOS Black Metal Matte,1,1,"Electro-mechanical profile for recessed installations in plasterboard ceilings, with 1m to 3m lengths.",0.000000000000,0.000000000000
1500 mm,48.000000000000,http://architectural.flos.com/professional/es/productos/sistemas_generales/the_fast_track,End Caps 08.9070.14 not included. To be ordered separately.,1500.000000000000,06.1851.14,FLOS,26 51 13,FLOS Black Metal Matte,1,1,"Electro-mechanical profile for recessed installations in plasterboard ceilings, with 1m to 3m lengths.",0.000000000000,0.000000000000
3000 mm,48.000000000000,http://architectural.flos.com/professional/es/productos/sistemas_generales/the_fast_track,End Caps 08.9070.14 not included. To be ordered separately.,3000.000000000000,06.1853.14,FLOS,26 51 13,FLOS Black Metal Matte,1,1,"Electro-mechanical profile for recessed installations in plasterboard ceilings, with 1m to 3m lengths.",0.000000000000,0.000000000000
